# 3D Printing Summary

|  |  |
| --- | --- |
| **Metrics** | **Single Row Playing Cards Holder** |
| Total Print Time (min) | 283 |
| Total Number of Components | 1 |
| Typical Total Mass (g) | 35 |
| Typical Number of Print Setups | 1 |

# 3D Printing Settings

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Print File Name** | **Qty** | **Total Print Time (hr:min)** | **Mass (g)** | **Infill (%)** | **Support(Y/N)** | **Layer Height/ Nozzle Diameter(mm)** | **Notes (orientation, special settings, etc.)** |
| Card\_Holder.stl | 1 | 4:43 | 35 | 15 | N | 0.2/0.4 | -Scale and rotate to fit printer bed  -Do not scale below 85% |

# Customization Options

Users may request their choice of print colour.

# Post-Processing

No post-processing is required as this print does not require supports. Rather inspect the print to ensure that all edges and surfaces are smooth.

# Examples of Quality Prints

